Contents

[Disable Bluetooth Services 1](#_Toc192510072)

[check that /dev/ttyAMA0 is now free: 1](#_Toc192510073)

[Check Available Serial Ports 1](#_Toc192510074)

## Disable Bluetooth Services

Now, stop and disable the **Bluetooth service** so it doesn’t restart:

sh

sudo systemctl stop hciuart.service

sudo systemctl disable hciuart.service

sudo reboot

## check that /dev/ttyAMA0 is now free:

sh

CopyEdit

sudo lsof /dev/ttyAMA0

## Check Available Serial Ports

Run:

sh

ls -l /dev/serial\*

## demo med Arduino

<https://www.diymachines.co.uk/tsx0108e-logic-level-converter>